**BLOCK DIAGRAM**

BUTTON PRESS

TEMPREATURE SENSOR ACTIVATED(Led on)

MONITORING OF TEMP

(ATMEGA328)

VALUE ON SERIAL MONITOR()

TEMPREATURE DETECTION